<http://ccm.net/faq/2144-how-to-use-network-bridge-wifi-bridge>

* In a DOS window, type the following command Run CMD as Administrator:

netsh bridge show adapter

Locate the card number responding when the bridge is active. If he says that your card is not in compatibility mode then do this: 

netsh bridge set adapter x forcecompatmode=enable

Replace x by number of your card displayed following the previous command.